|  |  |  |  |
| --- | --- | --- | --- |
| cit-bw | Corporate Finance Department Purchasing Division |  | |
|  |  | 791-2024 (Bid/Proposal No.) ADDENDUM 01 (Addendum No.) | |
|  |  | **Bus shelter polycarbonate glazing pilot project - Supply and Delivery of Polycarbonate Glazing material *(Contract Title)*** | |
|  | | | ISSUED: 2024-12-05 *(date)* |
|  | | | BY: James Marnoch *(name)* |
| URGENT **PLEASE FORWARD THIS DOCUMENT TO WHOEVER IS IN POSSESSION OF THE Bid/Proposal** | | | TELEPHONE NO. 204 226-3224 |
|  | | | THIS ADDENDUM SHALL BE INCORPORATED INTO THE BID/PROPOSAL AND SHALL FORM A PART OF THE CONTRACT DOCUMENTS  Template Version: Add 2024-02-01 |
|  | Please note the following and attached changes, corrections, additions, deletions, information and/or instructions in connection with the Bid/Proposal, and be governed accordingly. Failure to acknowledge receipt of this Addendum in Paragraph 10 of Form A: Bid/Proposal may render your Bid/Proposal non-responsive. | | | | |  |
|  |  | | | | |  |

**SPEC NOTE: Specify changes in the sequential order of the document.**

#### FORM B: PRICES

Replace: 791-2024 Form B: Prices with 791-2024 Addendum 01 - Form B: Prices. The following is a summary of changes incorporated in the replacement Bid/Proposal Submission:

Eg. Replace: 144-2006 Form B: Prices with 144-2006 **Addendum 1** Form B: Prices

Form B(R1): Revised Item #1 & Item #4 descriptions.

Revised the Total Bid Price formula to exclude Item #6 and #7.

Add Item #6 and #7 Spec. References and Item #6 Unit of Measure.

#### PART E – SPECIFICATIONS

Revise: E1.2 to read: The following are applicable to the Work:

SPEC NOTE: List all specifications, provided as separate documents, which apply. Do not list specifications included within this document.

|  |  |
| --- | --- |
| Specification No. | Specification Title |
| Table of Content |  |
| Item No. 1 | 1118mm X 2083mm X12mm thickness **OR** 1118mm X 2000mm X 12mm, edges finished for safe handling |
| Item No. 2 | 902mm X 2045mm X 12mm thickness, edges finished for safe handling |
| Item No. 3 | 902mm X 2083mm X 12mm thickness, edges finished for safe handling |
| Item No. 4 | 711mm X 2083 X 12mm thickness **OR** 711mm X 2000mm X 12mm, edges finished for safe handling |
| Item No. 5 | 2000mm X 3000mm X 12mm thickness, un-cut sheets |

SPEC NOTE: Insert revised clause in its entirety.

Revise: E2.2 to read: Item No. 1 – 1118mm X 2083mm X12mm thickness **OR** 1118mm X 2000mm X 12mm, edges finished for safe handling, edges finished for safe handling.

SPEC NOTE: Insert new clause.

Revise: E2.5 to read: Item No. 4 – 711mm X 2083 X 12mm thickness **OR** 711mm X 2000mm X 12mm, edges finished for safe handling.

SPEC NOTE: When replacing a form, make sure to **add the addendum number in the header and add the revision number (R#)** to the form that’s being replaced. See example below:

